**(SUB PAGE)**

**STANCOR U6K Chem-Resist Submersible Pump Technical Data – the Minion!**

|  |  |
| --- | --- |
| * Silicon carbide mechanical seal allows “dry” running. * Class B insulation. * Continuous operation to 140˚F if fully immersed * Plastic pump body, cover and impeller | * Strainer base, open impeller (10mm solids handling), 1 ¼” MPT discharge. * Aavailable with built-in level switch for fixed differential automatic level control if needed. |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Model** | **Voltage** | **Motor** | **RPM** | **kW Input** | **FLA** | **Thermal Protection** | **Weight**  (lbs) |
| U6K-E(S) | 115 or 220 | 75 HP | 3600 | 800 | 7/4 Amp | Built-in | 14.5 |
| U6K-D(S) | 230 or 460 | 75 HP | 3600 | 800 | 2.2 / 1.2 Amp | Built-in | 14.5 |

|  |  |
| --- | --- |
| ***Phone:480-998-4097***  [sales@apewater.com](mailto:sales@apewater.com) |  |