**WEBTROL NV280 Vertical Multistage Booster Pumps SPECIFICATIONS**

The Webtrol NV Series vertical multi-stage booster pumps offer stainless steel pump designs to meet a wide range of industrial process, commercial and agricultural applications. Booster pump bases and flange sizes allow drop in replacement for other brand pumps.

**304 Stainless Steel Pumps**

* All wetted parts are 304 or 316 SS.
* Standard WEG Motors. (ask us about other brands)
* Handles temperatures to 248 F, ideal for hot water process applications.
* Standard cartridge-type mechanical seals.
* Pump design enables standard electric C-Face motors.
* Heavy duty stainless steel hex shaft with stainless steel coupling.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Model:** | **Motor HP:** | **Motor Frame:** | **Pump Length:**  *(Pump only, in.)* | **Weight**  **Pump End:**  *(lbs.)* | **Length:**  *(WEG TEFC Motor only, in.)* | **Weight:**  *(WEG TEFC Motor only, lbs.)* |
| **NV280B1-1** | 7.5 | 213TC | 22.36 | 116 | 19” | 152 |
| **NV280B1** | 15 | 254TC | 26.50 | 137 | 25” | 278 |
| **NV280B2-2** | 15 | 254TC | 29.74 | 145 | 25” | 278 |
| **NV280B2-1** | 20 | 254TC | 29.74 | 145 | 26.7” | 315 |
| **NV280B2** | 25 | 284.TSC | 29.74 | 148 | 27” | 383 |
| **NV280B3-2** | 30 | 286TSC | 32.99 | 156 | 30” | 484 |
| **NV280B3-1** | 40 | 286TSC | 32.99 | 156 | 30.7” | 570 |
| **NV280B3** | 40 | 286TSC | 32.99 | 156 | 30.7” | 570 |
| **NV280B4-2** | 40 | 286TSC | 36.24 | 164 | 30.7” | 570 |
| **NV280B4-1** | 50 | 326TSC | 36.24 | 182 | 33.7” | 474 |
| **NV280B4** | 50 | 326TSC | 36.24 | 182 | 33.7” | 474 |
| **NV280B5-2** | 60 | 364TSC | 39.49 | 182 | 37.4” | 1,047 |
|  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| 9332 North 95th Way  Scottsdale, AZ 85258  ***Phone:480-998-4097***  [sales@apewater.com](mailto:sales@apewater.com) |  |