**WEBTROL NV400 Vertical Multistage Booster Pumps SPECIFICATIONS**

The Webtrol NV Series vertical multi-stage booster pumps offer stainless steel pump designs to meet a wide range of industrial process, commercial and agricultural applications. Booster pump bases and flange sizes allow drop in replacement for other brand pumps.

**304 Stainless Steel Pumps**

* All wetted parts are 304 or 316 SS.
* Standard WEG Motors. (ask us about other brands)
* Handles temperatures to 248 F, ideal for hot water process applications.
* Standard cartridge-type mechanical seals.
* Pump design enables standard electric C-Face motors.
* Heavy duty stainless steel hex shaft with stainless steel coupling.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Model:** | **Motor HP:** | **Motor Frame:** | **Pump Length:***(Pump only, in.)* | **Weight** **Pump End:***(lbs.)* | **Length:** *(WEG TEFC Motor only, in.)* | **Weight:***(WEG TEFC Motor only, lbs.)* |
| **NV400B1-1** | 15 | 254TC | 26.75 | 160 | 25” | 278 |
| **NV400B1** | 15 | 254TC | 26.75 | 160 | 25” | 278 |
| **NV400B2-2** | 25 | 284TSC | 30.34 | 173 | 27” | 383 |
| **NV400B2-1** | 30 | 286TSC | 30.34 | 173 | 30” | 484 |
| **NV400B2** | 40 | 286TSC | 30.34 | 173 | 30.7” | 570 |
| **NV400B3-2** | 40 | 286TSC | 33.93 | 184 | 30.7” | 570 |
| **NV400B3-1** | 50 | 326TSC | 33.93 | 202 | 33.7” | 474 |
| **NV400B3** | 50 | 326TSC | 33.93 | 202 | 33.7” | 474 |
| **NV400B4-2** | 60 | 364TSC | 37.36 | 217 | 37.4” | 1,047 |
| **NV400B4-1** | 60 | 364TSC | 37.36 | 217 | 37.4” | 1,047 |
|  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| 9332 North 95th Way Scottsdale, AZ 85258 ***Phone:480-998-4097*** sales@apewater.com |  |