**WEBTROL NV45 Vertical Multistage Booster Pumps SPECIFICATIONS**

The Webtrol NV Series vertical multi-stage booster pumps offer stainless steel pump designs to meet a wide range of industrial process, commercial and agricultural applications. Booster pump bases and flange sizes allow drop in replacement for other brand pumps.

**304 Stainless Steel Pumps**

* All wetted parts are 304 or 316 SS.
* Standard WEG Motors. (ask us about other brands)
* Handles temperatures to 248 F, ideal for hot water process applications.
* Standard cartridge-type mechanical seals.
* Pump design enables standard electric C-Face motors.
* Heavy duty stainless steel hex shaft with stainless steel coupling.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Model:** | **Motor HP:** | **Motor Frame:** | **Pump Length:***(Pump only, in.)* | **Weight** **Pump End:***(lbs.)* | **Length:** *(WEG TEFC Motor only, in.)* | **Weight:***(WEG TEFC Motor only, lbs.)* |
| **NV45B1** | 1 | 56C | 14.96 | 60 | 13” | 42 |
| **NV45B2** | 1.5 | 56C | 14.96 | 60 | 13” | 48 |
| **NV45B3** | 3 | 182TC | 17.5 | 84 | 16” | 96 |
| **NV45B4** | 3 | 182TC | 18.35 | 87 | 16” | 96 |
| **NV45B5** | 5 | 182TC | 19.53 | 89 | 17” | 106 |
| **NV45B6** | 5 | 182TC | 20.71 | 91 | 17” | 106 |
| **NV45B7** | 5 | 182TC | 22.44 | 97 | 17” | 106 |
| **NV45B8** | 7.5 | 213TC | 23.62 | 99 | 19” | 152 |
| **NV45B9** | 7.5 | 213TC | 24.80 | 101 | 19” | 152 |
| **NV45B10** | 7.5 | 213TC | 25.98 | 104 | 19” | 152 |
| **NV45B12** | 10 | 213TC | 28.34 | 108 | 20.7” | 179 |
| **NV45B14** | 10 | 213TC | 33.33 | 126 | 20.7” | 179 |
| **NV45B16** | 15 | 254TC | 35.69 | 130 | 25” | 278 |
| **NV45B17** | 15 | 254TC | 38.06 | 133 | 25” | 278 |
|  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| 9332 North 95th Way Scottsdale, AZ 85258 ***Phone:480-998-4097*** sales@apewater.com |  |