**WEBTROL NV6 Vertical Multistage Booster Pumps SPECIFICATIONS**

The Webtrol NV Series vertical multi-stage booster pumps offer stainless steel pump designs to meet a wide range of industrial process, commercial and agricultural applications. Booster pump bases and flange sizes allow drop in replacement for other brand pumps.

**304 Stainless Steel Booster Pumps**

* All wetted parts are 304 or 316 SS.
* Standard WEG Motors. (ask us about other brands)
* Handles temperatures to 248 F, ideal for hot water process applications.
* Standard cartridge-type mechanical seals.
* Pump design enables standard electric C-Face motors.
* Heavy duty stainless steel hex shaft with stainless steel coupling.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Model:** | **Motor HP:** | **Motor Frame:** | **Pump Length:***(Pump only, in.)* | **Weight** **Pump End:***(lbs.)* | **Length:** *(WEG TEFC Motor only, in.)* | **Weight:***(WEG TEFC Motor only, lbs.)* |
| **NV6B2** | .33 | 56C | 12.05 | 31 | 12” | 36 |
| **NV6B3** | .33 | 56C | 12.05 | 31 | 12” | 36 |
| **NV6B4** | .5 | 56C | 12.76 | 32 | 12” | 40 |
| **NV6B5** | .5 | 56C | 13.46 | 32 | 12” | 40 |
| **NV6B6** | .75 | 56C | 14.17 | 33 | 12” | 41 |
| **NV6B7** | .75 | 56C | 14.84 | 34 | 12” | 41 |
| **NV6B8** | 1 | 56C | 15.55 | 35 | 13” | 42 |
| **NV6B9** | 1 | 56C | 16.26 | 35 | 13” | 42 |
| **NV6B10** | 1 | 56C | 16.97 | 36 | 13” | 42 |
| **NV6B11** | 1.5 | 56C | 17.68 | 37 | 13” | 48 |
| **NV6B12** | 1.5 | 56C | 18.39 | 38 | 13” | 48 |
| **NV6B13** | 1.5 | 56C | 19.09 | 39 | 13” | 48 |
| **NV6B15** | 2 | 56C | 20.55 | 41 | 14” | 56 |
| **NV6B17** | 2 | 56C | 21.97 | 43 | 14” | 56 |
| **NV6B19** | 2 | 56C | 24.31 | 49 | 14” | 56 |
| **NV6B21** | 3 | 182TC | 25.73 | 51 | 16” | 96 |
| **NV6B23** | 3 | 182TC | 27.15 | 53 | 16” | 96 |
| **NV6B25** | 3 | 182TC | 28.56 | 54 | 16” | 96 |
| **NV6B27** | 3 | 182TC | 29.98 | 56 | 16” | 96 |

|  |  |
| --- | --- |
| 9332 North 95th Way Scottsdale, AZ 85258 ***Phone:480-998-4097*** sales@apewater.com |  |