**WEBTROL NV65 Vertical Multistage Booster Pumps SPECIFICATIONS**

The Webtrol NV Series vertical multi-stage booster pumps offer stainless steel pump designs to meet a wide range of industrial process, commercial and agricultural applications. Booster pump bases and flange sizes allow drop in replacement for other brand pumps.

**304 Stainless Steel Pumps**

* All wetted parts are 304 or 316 SS.
* Standard WEG Motors. (ask us about other brands)
* Handles temperatures to 248 F, ideal for hot water process applications.
* Standard cartridge-type mechanical seals.
* Pump design enables standard electric C-Face motors.
* Heavy duty stainless steel hex shaft with stainless steel coupling.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Model:** | **Motor HP:** | **Motor Frame:** | **Pump Length:***(Pump only, in.)* | **Weight** **Pump End:***(lbs.)* | **Length:** *(WEG TEFC Motor only, in.)* | **Weight:***(WEG TEFC Motor only, lbs.)* |
| **NV65B1** | 2 | 56C | 16.10 | 62 | 14” | 56 |
| **NV65B2** | 5 | 182TC | 17.13 | 84 | 17” | 106 |
| **NV65B3** | 5 | 182TC | 19.49 | 91 | 17” | 106 |
| **NV65B4** | 7.5 | 213TC | 21.22 | 94 | 19” | 152 |
| **NV65B5** | 10 | 213TC | 22.99 | 97 | 20.7” | 179 |
| **NV65B6** | 10 | 213TC | 27.39 | 114 | 20.7” | 179 |
| **NV65B7** | 15 | 254TC | 29.16 | 117 | 25” | 278 |
| **NV65B8** | 15 | 254TC | 30.93 | 120 | 25” | 278 |
| **NV65B9** | 15 | 254TC | 32.70 | 123 | 25” | 278 |
| **NV65B10** | 20 | 254TC | 34.47 | 126 | 26.7” | 315 |
| **NV65B12** | 25 | 284TSC | 37.26 | 126 | 27” | 383 |
|  |  |  |  |  |  |  |

|  |  |
| --- | --- |
| 9332 North 95th Way Scottsdale, AZ 85258 ***Phone:480-998-4097*** sales@apewater.com |  |