**STANCOR Oil Minder Elevator Pump Technical Data and Specifications**

OIL Minder® elevator pit pump systems are specifically designed for sump applications where it is critical to pump water, but leave potentially harmful oils behind. Oil Minder® Systems are widely used as hydraulic elevator sump pumps to prevent leaked hydraulic oil from being pumped into the wastewater discharge. Easy to install plug-in systems, in simplex or duplex configurations for elevator pits, transformer vaults, industrial sumps.

**Now Offering Elevator Sump Pumps with BACnet!**

Oil Minder® systems were recently enhanced with BACnet automation capability to combine plumbing and HVAC equipment into the same channel for alarms, fault codes and operating schedules. This means equipment, like an elevator, can send status information through BACnet to create the backbone of a comprehensive maintenance program.

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **MODEL** | **HP** | **Phase** | **Voltage** | **Amps**  (FLA) | **RPM** | **Disch.**  (NPT) | **Head @ 50 GPM** | **Head @ 100 GPM** | **Weight**  (lbs) | **Height** | **Width** |
| **SE40** | **.04** | 1 | 115 | 5.2 | 3,450 | 2” | 11 | --- | 24 | 15.59” | 9.09” |
| 208 | 2.9 |
| 230 | 2.6 |
| 3 | 208 | 2.2 |
| 230 | 2 |
| 460 | 1 |
| 575 | 0.8 |
| **SE50** | **.05** | 1 | 115 | 8 | 3,450 | 2” | 22 | --- | 29 | 16.57” | 9.09” |
| 208 | 4.4 |
| 230 | 4 |
| 3 | 208 | 3.1 |
| 230 | 2.8 |
| 460 | 1.4 |
| 575 | 1.2 |
| **SE100** | **1.0** | 1 | 115 | 12 | 3,450 | 2” | 33 | 9 | 40 | 19.53” | 9.09” |
| 208 | 6.6 |
| 230 | 6 |
| 3 | 208 | 4.4 | 3,450 | 2” | 36 | 14 |
| 230 | 4 |
| 460 | 2 |
| 575 | 1.6 |