**STANCOR SKR Heavy Duty Slurry Pump Specifications**

|  |  |  |
| --- | --- | --- |
| * Wet end components constructed in high-chromium alloy steel.
* 1800 RPM motors with class F motor insulation
 | * Double mechanical seals
* 410 Stainless steel rotor and shaft sleeve
* Housing with integrated cooling jacket
 | * High chrome steel semi-vortex impellers
* Heavy duty 5-conductor cables
 |
| **MODEL** | **HP** | **Voltage** | **Amps**(FLA) | **Discharge**(NPT) | **Max Solids**(in) | **Max Flow**GPM | **Max Head** (Ft) | **Weight**(lbs) | **Dimensions** |
| **SKR-337-230** | 5 | 230 | 15.0 | 3” | 1" | 340 | 50 | 242 | 31 H /15.1 W |
| **SKR-337-460** | 5 | 460 | 7.7 | 3” | 1" | 340 | 50 | 242 | 31 H /15.1 W |
| **SKR-337-460** | 5 | 575 | 6.3 | 3” | 1" | 340 | 50 | 242 | 31 H /15.1 W |
| **SKR-437-230** | 5 | 230 | 15.0 | 4” | 1" | 515 | 52 | 242 | 31 H /15.1 W |
| **SKR-437-460** | 5 | 460 | 7.7 | 4” | 1" | 515 | 52 | 242 | 31 H /15.1 W |
| **SKR-437-460** | 5 | 575 | 6.3 | 4” | 1" | 515 | 52 | 242 | 31 H /15.1 W |
| **SKR-355-230** | 7.5 | 230 | 22.6 | 3” | 1" | 580 | 66 | 271 | 31 H /16.3 W |
| **SKR-355-460** | 7.5 | 460 | 11.5 | 3” | 1" | 580 | 66 | 271 | 31 H /16.3 W |
| **SKR-355-460** | 7.5 | 575 | 9.2 | 3” | 1" | 580 | 66 | 271 | 31 H /16.3 W |
| **SKR-455-230** | 7.5 | 230 | 22.6 | 4” | 1" | 595 | 62 | 273 | 31 H /16.3 W |
| **SKR-455-460** | 7.5 | 460 | 11.5 | 4” | 1" | 595 | 62 | 273 | 31 H /16.3 W |
| **SKR-455-460** | 7.5 | 575 | 9.2 | 4” | 1" | 595 | 62 | 273 | 31 H /16.3 W |
| **SKR-475-230** | 10 | 230 | 30.1 | 4”  | 1" | 620 | 70 | 273 | 31 H /16.3 W |
| **SKR-475-460** | 10 | 460 | 15.0 | 4” | 1" | 620 | 70 | 273 | 31 H /16.3 W |
| **SKR-475-460** | 10 | 575 | 12.2 | 4” | 1" | 620 | 70 | 273 | 31 H /16.3 W |
| **SKR-4110-230** | 15 | 230 | 45.2 | 4” | 1" | 780 | 85 | 421 | 35.8 H /18.8 W |
| **SKR-4110-460** | 15 | 460 | 22.6 | 4” | 1" | 780 | 85 | 421 | 35.8 H /18.8 W |
| **SKR-4110-460** | 15 | 575 | 17.9 | 4” | 1" | 780 | 85 | 421 | 35.8 H /18.8 W |
| **SKR-6110-230** | 15 | 230 | 45.2 | 6” | 1 3/8" | 1050 | 80 | 423 | 35.8 H /18.8 W |
| **SKR-6110-460** | 15 | 460 | 22.6 | 6” | 1 3/8" | 1050 | 80 | 423 | 35.8 H /18.8 W |
| **SKR-6110-460** | 15 | 575 | 17.9 | 6” | 1 3/8" | 1050 | 80 | 423 | 35.8 H /18.8 W |
| **SKR-6150-230** | 20 | 230 | 60.3 | 6” | 1.5" | 1135 | 100 | 443 | 35.8 H /18.8 W |
| **SKR-6150-460** | 20 | 460 | 30.1 | 6” | 1.5" | 1135 | 100 | 443 | 35.8 H /18.8 W |
| **SKR-6150-460** | 20 | 575 | 24.1 | 6” | 1.5" | 1135 | 100 | 443 | 35.8 H /18.8 W |
| **SKR-6220-460** | 30 | 460 | 45.2 | 6” | 1.5" | 1240 | 108 | 761 | 45.1 H /23.3 W |
| **SKR-6220-460** | 30 | 575 | 36.2 | 6” | 1.5" | 1240 | 108 | 761 | 45.1 H /23.3 W |
| **SKR-8220-460** | 30 | 460 | 45.2 | 8” | 1.5" | 1640 | 82 | 783 | 45.1 H /23.3 W |
| **SKR-8220-460** | 30 | 575 | 36.2 | 8” | 1.5" | 1640 | 82 | 783 | 45.1 H/23.3 W |