**WEBTROL NV25 Vertical Multistage Booster Pumps SPECIFICATIONS**

The Webtrol NV Series vertical multi-stage booster pumps offer stainless steel pump designs to meet a wide range of industrial process, commercial and agricultural applications. Booster pump bases and flange sizes allow drop in replacement for other brand pumps.

**304 Stainless Steel Pumps**

* All wetted parts are 304 or 316 SS.
* Standard WEG Motors. (ask us about other brands)
* Handles temperatures to 248 F, ideal for hot water process applications.
* Standard cartridge-type mechanical seals.
* Pump design enables standard electric C-Face motors.
* Heavy duty stainless steel hex shaft with stainless steel coupling.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Model:** | **Motor HP:** | **Motor Frame:** | **Pump Length:**  *(Pump only, in.)* | **Weight**  **Pump End:**  *(lbs.)* | **Length:**  *(WEG TEFC Motor only, in.)* | **Weight:**  *(WEG TEFC Motor only, lbs.)* |
| **NV25B2** | .75 | 56C | 11.93 | 33 | 12” | 41 |
| **NV25B3** | 1 | 56C | 13.10 | 35 | 13” | 42 |
| **NV25B4** | 1.5 | 56C | 14.06 | 36 | 13” | 48 |
| **NV25B5** | 1.5 | 56C | 15.12 | 38 | 13” | 48 |
| **NV25B6** | 2 | 56C | 16.28 | 39 | 14” | 56 |
| **NV25B7** | 2 | 56C | 18.29 | 45 | 14” | 56 |
| **NV25B8** | 3 | 182TC | 19.35 | 46 | 16” | 96 |
| **NV25B9** | 3 | 182TC | 20.31 | 47 | 16” | 96 |
| **NV25B10** | 3 | 182TC | 21.44 | 49 | 16” | 96 |
| **NV25B11** | 5 | 182TC | 22.50 | 50 | 17” | 106 |
| **NV25B12** | 5 | 182TC | 23.56 | 51 | 17” | 106 |
| **NV25B13** | 5 | 182TC | 24.63 | 52 | 17” | 106 |
| **NV25B14** | 5 | 182TC | 25.69 | 53 | 17” | 106 |
| **NV25B15** | 5 | 182TC | 26.75 | 54 | 17” | 106 |
| **NV25B16** | 5 | 183TC | 27.82 | 56 | 17” | 106 |
| **NV25B18** | 7.5 | 213TC | 30.57 | 63 | 19” | 152 |
| **NV25B20** | 7.5 | 213TC | 32.70 | 66 | 19” | 152 |
| **NV25B22** | 7.5 | 213TC | 34.72 | 58 | 19” | 152 |
| **NV25B24** | 7.5 | 213TC | 36.85 | 70 | 19” | 152 |

|  |  |
| --- | --- |
| 9332 North 95th Way  Scottsdale, AZ 85258  ***Phone:480-998-4097***  [sales@apewater.com](mailto:sales@apewater.com) |  |