**PEMO Submersible Slurry Pumps Specifications**

**HARDALLOY Construction**

Available in single and Double Staged versions featuring:

|  |  |
| --- | --- |
| \* Impeller, volutes, sleeves, suction covers and discharge elbows all in hardalloy. \* Built-in thermal overload protection.\* Double mechanical seals. | \* Moisture detection.\* Heavy duty lip seals.\* Heavy duty thrust bearings\* Shafts made of 420 SS. |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Pump Model**  | **Power**(hp) | **Speed**(rpm) | **Max Flow**(gpm) | **Max Head**(ft) | **Discharge ø**(in) |
| **S-FP** | 5.5 to 25 | 1750-3500 | 260 | 190 | 2.5 |
| **603-H** | 15 to 40 | 1750-3500 | 550 | 165 | 3 |
| **K125-H** | 15 to 50 | 1150-1750 | 660 | 165 | 3 |
| **1004-H** | 25 to 60 | 880-1150 | 1300 | 130 | 4 |
| **1706/99-H** | 40 to 75 | 880-1150 | 1600 | 120 | 6 |

**RUBBER LINED Construction**

Designed for heavy duty slurry applications featuring:

|  |  |
| --- | --- |
| \* Rubber lined casings with Hardalloy impellers. \* Mechanical seals made of silica or tungsten carbide.  | \* Thermal probes for motor temperature control. \* Oil level probes for slurry leak detection in the oil chamber. |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Pump Model**  | **Power***(hp)* | **Speed***(rpm)* | **Max Flow***(gpm)* | **Max Head***(ft)* | **Discharge ø***(in)* |
| **33** | 1.5 to 4 | 1750-3500 | 80 | 65 | 1 |
| **302** | 3 to 4 | 1750-3500 | 100 | 65 | 1.5 |
| **403** | 5.5 to 12 | 1750-3500 | 180 | 100 | 2 |
| **503** | 5.5 to 25 | 1750-3500 | 220 | 150 | 2.5 |
| **533** | 5.5 to 25 | 1750-3500 | 400 | 150 | 3 |
| **603** | 15 to 40 | 1750-3500 | 480 | 165 | 3 |
| **804** | 15 to 30 | 1750-3500 | 660 | 85 | 3 |
| **K125** | 25 to 50 | 1150-1750 | 660 | 165 | 3 |
| **1004** | 25 to 60 | 1150-1750 | 1000 | 130 | 4 |
| **1706/99** | 40 to 75 | 880-1150 | 1600 | 120 | 6 |
| **G230** | 40 to 100 | 880-1150 | 2400 | 120 | 8 |
| **I-270** | 60 to 150 | 880-1150 | 3200 | 120 | 8 |

|  |  |
| --- | --- |
| 9332 North 95th Way Scottsdale, AZ 85258 ***Phone:480-998-4097*** sales@apewater.com |  |